Yes, it is possible with Automation feature. In the attachment you will printscreen where is Helios IP set as you requested.

When Helios IP receive code "12345\*" in the call, then he will switch to external camera.

When Helios IP receive code "54321\*" in the call, then he will switch to internal camera.

